

System requirements for PROBE_GatewayPC software:
PC with Windows 98/NT/2000/XP/7/10 system.

Uninstall previous version of GatewayPC software from your system 
(Add/Remove programs in Control Panel).


1. Click on SETUP.EXE to install PROBE_GatewayPC software.
2. Click on START button and select PROBE_GatewayPC program group.  
    
The following applications are installed in this group:
- PROBE_GatewayPC application for sensor display, monitoring, calibration and data   
  collection in MS Excel format.
- Profile Viewer to view probe profile.
- DownloadToPic application to download probe "hex" file.
- MiniProbe application for mini probe monitoring and calibration.


Changes for Version 6.3

1) In Tools when ultrasonic sensor is installed in the middle of the
dome shape tank which creates multiply reflections, please select
Middle Tank Installation and turn it ON. This parameter can also be
turned ON by pressing the push-button of the sensor and realising it
after the LED light is OFF.

2) In Tools Power coef. is used to increase power of the radar which
can help in case of multiply reflections and unwanted echoes from oilwater
and oil-tank bottom interfaces, this feature is recommended with
Low Dielectric Material OFF and 20mA Blanking is OFF. The Power coef.
equal to 40 turns on the logic to handle roof reflection problem and
oil-water separation false echo.

3) In Tools Distance to Target is used for solid materials during
start-up when radar doesn't receive any echoes. Click on this
parameter and put a distance from the radar mounting thread to surface
of solid material. Radar will display that distance until valid echoes
will be received, Probe Software Rev. 14 is required (find it in
ShowCaliData).

4) In Tools Select Data Link Speed selects two Baud Rates 9600 or
19.2K for communication with level sensors. After speed selection
click on Stop Data Link, and close the communication program and restart
it again.

5) In Applications there are the following options: Oil Application,
Mini Probe (described in point 17), BASE_TANK_Farm and

CUSTOM_TANK_Farm.

a) Oil APPlication, select it when Oil-water interface is downloadedto the radar and please follow the instruction:

1) In Tools do 4mA and 20mA calibration.
2) Click on Applications and choose Oil Application.
3) You get displayed on the screen: Oil Thickness, first value is the
timer, second is the thickness in Inches, plus you get Oil Dielectric
Constant display.
4) Click on Tools and choose Oil Dielectric Constant, enter value for
dielectric constant of oil (clean oil is about 2, crude one about 3 or4)
5) Click on Send to Probe, wait for the conformation and Exit this
feature.
6) Click Stop Data Link and close completely GatewayPC.
7) Open again the GatewayPC and repeat point 2.
8) In Tools click on Oil App Tuning, choose about 20sec.
9) You will get on the screen two current values, one from the oil top
and another one from oil-water interface, the hardware current from
the radar will display the same two values. The current output will
alternate between top of oil and oil-water interface every 20sec (this
time is set up by OIL App Tuning).

b) BASE_TANK_Farm, select it when a tank graphical display is
required, choose your tank shape, click on Build Custom Tank, fill
out Tank Data, Tank ID is the one selected in ProbeGatewayPC_Net.
Empty Tank Calibration can't be longer than TANK HEIGHT. After that
click on Save, this will be saved and it will be listed on
CUSTOM_TANK_Farm by Tank's Name and ID and displayed as bar graphs.
Next to each bar graph, level in %, material name, tank's free space
and distance from sensor to material surface are also displayed. A
tank will be fully displayed by clicking on tank list. In
CUSTOM_