; Windows INF File for a USB virtual COM-port device
; in the communication devices class (CDC)


[Version]
Signature="$Windows NT$" 
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
LayoutFile=layout.inf
DriverVer=06/05/2015,5.1.2600.0
CatalogFile =OmegaVCP.cat


[Manufacturer]
%MFGNAME%=DeviceList ,NTx86, NTamd64

[DestinationDirs]
DefaultDestDir=12
DriverCopyFiles=12


[DeviceList.NTx86]
%DESCRIPTION%=DriverInstall, USB\VID_2A72&PID_0400

[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_2A72&PID_0400

[DeviceList.NTia64]
%DESCRIPTION%=DriverInstall, USB\VID_2A72&PID_0400

[DriverInstall.nt]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles
AddReg=DriverInstall.nt.AddReg
[DriverCopyFiles]
usbser.sys
[DriverInstall.nt.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
[DriverInstall.nt.Services]
include=mdmcpq.inf
AddService=usbser, 0x00000002, DriverService
[DriverService]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys
[Strings] 
MFGFILENAME="CDC"
DRIVERFILENAME="usbser"
Omega="Omega COM Port"
MFGNAME="Omega Engineering"
DESCRIPTION="USB COM Port" 
SERVICE="USB COM-port Driver"
ProviderName="Omega Engineering"